**Table 12:** MSR 1C1 nozzle #11 north loading

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Equipment ID → | | MSR 1C1 Nozzle #11 North | | | Allowable Load Reference → | | | Note 1 | |
| Equipment Dwg. | |  | | |  | | |  | |
| Attached Piping Data Summary | | | Computer Run ID | | | | Nozzle or Penetration Local Coordinate System | | |
| HSG Input | | | |
| NPS & Schedule: 8 / 40 | | | Note 1:  Allowable nozzle loads are not available for this nozzle. During MSR replacement, allowable loads will be established and included in this analysis. | | | | +X: Along nozzle axis, coming out of nozzle  +Y: Toward plant South  +Z: Determined by right-hand-rule | | |
| Pipe Material: Carbon Steel A106-B | | |
| Metal Area (in2): 8.4 | | |
| Section Modulus (in3): 16.81 | | |
| Load | | FAX | FS1 | FS2 | FSR | MTOR | MB1 | MB2 | MBR |
| Local Coordinate ID | | FX | FY | FZ |  | MX | MY | MZ |  |
| LB | LB | LB | LB | FT-LB | FT-LB | FT-LB | FT-LB |
| **NORMAL** | Dead Weight |  |  |  |  |  |  |  |  |
| TH-1 |  |  |  |  |  |  |  |  |
| TH-2 |  |  |  |  |  |  |  |  |
| Hot (weight + envelope of expansion cases) |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Maximum of the Absolute Value of (DW, Hot) |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Allowable | Note 1 |  |  | Note 1 | Note 1 |  |  | Note 1 |
| Ratio | -- |  |  | -- | -- |  |  | -- |